# Trade Mark Journal No.2026/024 12 June 2026

## WO0000001920149 (9,17,37,41,42)

Office of origin: Germany

Date of International Registration:1 April 2026
Date of designation in the UK: 1 April 2026

Light blue and dark blue.

Characters “DRIESCHER” are in dark blue; Characters “WD” as well as “wegberg” are in light blue; Background is in white.

Class 9
  Electrical and mechanical switches and systems containing electrical and mechanical switches for the distribution of electrical energy, in particular electrical switching devices including load switches, load break switches, and circuit breakers; switchgear for high- and medium-voltage distribution systems, including those for power distribution systems operating at rated voltages exceeding 1000 volts; SF6 (sulfur hexafluoride) - insulated load breaking and circuit breaking switchgear; F-gas (fluor containing gas) - free load breaking and circuit breaking switchgear; air-insulated load breaking and circuit breaking switchgear; solid-insulated load breaking and circuit breaking switchgear; plastic and concrete substations [transformers]; electrical testing systems consisting of software for testing electrical switchgear; electrical testing instruments; electrical testing equipment for power grids; devices for testing electrical power systems.
Class 17
  Electrical insulators, in particular made of cast resin and/or ceramic, in particular for use at rated voltages exceeding 1000 volts.
Class 37
  Installation and maintenance of electrical and mechanical switches and systems containing electrical and mechanical switches for the distribution of electrical energy, in particular electrical switching devices including load switches, load break switches, and circuit breakers, of switchgear for high- and medium-voltage distribution systems, including switchgear for high- and medium-voltage distribution systems, including those for power distribution systems operating at rated voltages exceeding 1000 volts, of SF6 (sulfur hexafluoride) -insulated load breaking and circuit breaking switchgear, of F-gas (fluor containing gas) - free load breaking and circuit breaking switchgear, of air-insulated load breaking and circuit breaking switchgear, of solid-insulated load breaking and circuit breaking switchgear, and of plastic and concrete substations [transformers]; maintenance of electrical testing systems [hardware] for electrical switchgear, electrical test instruments, electrical testing equipment for power grids, and devices for testing electrical power systems.
Class 41
  Organization and hosting of seminars and training courses in the field of safety, particularly in connection with electrical and mechanical switches and systems comprising electrical and mechanical switches for the distribution of electrical energy.
Class 42
  Technical consulting in the field of safety, particularly in connection with the operation of electrical and mechanical switches and systems comprising electrical and mechanical switches for the distribution of electrical energy, particularly electrical switchgear including load switches, load break switches and circuit breakers, switchgear for high-and medium-voltage distribution systems, including power distribution systems operated at rated voltages exceeding 1,000 volts, SF6 (sulfur hexafluoride) -insulated load and circuit breaker systems, F-gas (fluor containing gas) - free load breaking and circuit breaking switchgear, air-insulated load breaking and circuit breaking switchgear, solid-insulated load breaking and circuit breaking switchgear, as well as plastic and concrete substations; development of new technical products for third parties in the field of electrical and mechanical switches and systems comprising electrical and mechanical switches for the distribution of electrical energy, in particular electrical switchgear, including load switches, load break switches and circuit breakers, switchgear cells for high- and medium voltage distribution systems, including power distribution systems operating at rated voltages exceeding 1,000 volts, SF6 (sulfur hexafluoride) - insulated load breaking and circuit breaking switchgear, F-gas (fluor containing gas) - free load breaking and circuit breaking switchgear, air-insulated load breaking and circuit breaking switchgear, solid-insulated load breaking and circuit breaking switchgear, as well as plastic and concrete substations; development of new technical products related to electrical testing systems for electrical switchgear, electrical test instruments, electrical test equipment for power grids, and devices for testing electrical power systems; development of new technical products related to electrical insulators made primarily of cast resin and/or ceramics, particularly for use at rated voltages exceeding 1,000 volts.

Fritz Driescher KG Spezialfabrik für Elektrizitätswerksbedarf GmbH & Co.

Representative: LENZING GERBER STUTE Partnerschaftsgesellschaft von Patentanwälten m.b.B., Bahnstraße 9, 40212 Düsseldorf, GERMANY