# Trade Mark Journal No.2026/007 13 February 2026

## UK00004330948 27 January 2026 (6,12)

Mark 1

Mark 2

International priority date claimed: 29 July 2025 (United States of America) (99307940)
International priority date claimed: 29 July 2025 (United States of America) (99307941)

Class 6
  Metal hardware for supporting flexible air brake hoses between rail cars, namely, hangers, connectors, and brackets. Floor and walk metal grating, namely, walkways, platforms, steps and catwalks; Metal safety grating, namely, walkways, platforms, steps and catwalks. Brake beams and parts thereof all being for use on railway cars.
Class 12
  Side bearings, roller side bearings, snubbers, hydraulic stabilizers, resilient side bearings and friction shoes and parts thereof all being for use on railway cars. Friction suspension assemblies for railway cars and components thereof comprising elastomeric pads, coil springs, metal wear plates and wedges. Motion control units for railway cars, namely, side bearings and snubbers and parts thereof. Resilient friction dampeners for railway vehicles, including resilient side bearings and friction shoes. Friction dampening devices, namely, side bearings and dampeners for railway vehicles. Constant contact side bearings for railway vehicles. Draft gear for railway vehicles; friction draft gear for railway vehicles; high capacity friction draft gear for railway vehicles. Discharge gates for railroad freight cars. Roller bearing backing rings for railcar axles; universal roller bearing backing rings for railcar axles; railway backing rings for railcar axles; universal railway backing rings for railcar axles; backing rings for railcar axles; universal backing rings for railcar axles. Suspension springs for railroad cars and locomotives. Railroad car equipment, namely, handles, handle extensions and handle latches for opening, closing and latching outlet valves on the bottom of railroad tank cars. Railroad car equipment, namely vented and non-vented hatch covers, vented outlet caps, manway covers, vacuum relief devices, gauge devices, eduction tubes, top and bottom unloading adapters, and secondary closures, namely, plugs, caps and blind flanges, used in the transport, loading, and unloading of railroad tank and hopper cars.

A. Stucki Company

Representative: Mishcon de Reya LLP